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	PRODUCT REPORT CARD

	J30-40XMT2
	HYSTER

	INCREASED PRODUCTIVITY
	

	 Vista Mast and open face integral carriage design
	

	 Seat side hydraulics
	

	 Hydrostatic steer system
	

	 SEM traction control system
	

	REDUCED MAINTENANCE COSTS
	

	 Chrome plated cylinder rods
	 

	 Hydrostatic steer system
	 

	 Rugged all welded steel constructed frame
	 

	 Regenerative braking
	 

	INCREASED OPERATOR COMFORT
	

	 Open / spacious operator compartment
	 

	 Five position tilt steering wheel / column
	 

	 Dual wheel steer axle
	 

	 Power Steering and Hoist motors are shock mounted 
	 

	RELIABILITY / DEPENDABILITY
	

	 Hydrostatic steer system
	 

	 Totally enclosed rack & pinion hydraulic steer axle assembly
	 

	 Traction controllers feature soldered electrical connections 
	 

	 Vista mast with canted load rollers 
	 

	SERVICEABILITY
	

	 Boltless two piece drop in floor plate
	 

	 Rearward pivoting hood with two gas assist cylinders 
	 

	 Standard dash display with LED warnings
	 

	 Full radius angled roller mast channel bearings
	 

	REDUCED PRODUCT DAMAGE
	

	 Hydrostatic steer system with dual steer wheels
	 

	 Pressure compensated lowering control valve
	 

	 Vista mast design \ open faced carriage 
	 

	 Bar on edge overhead guard design
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