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R30XM2 ORDERPICKER 
 POCKET GUIDE

Performance

· Standard HySense continuous height sensing optimizes maximum travel speed at various fork heights above 60.0” compared to conventional stepped speed traction systems. It gradually reduces travel speed at fork heights between 60.0” – 212.0”. 
· Widely spaced mast channels make it easier to see ahead for improved maneuvering in picking aisle.
· Separately excited motors allow ideal tractive performance for productivity.  
· 24-volt and optional 36-volt electrical system offers optimum power for handling capacity loads.
· Multi-function accelerator handle provides simultaneous command of variable lift/lower speed, travel direction, acceleration, and horn for great load handling efficiency.
· Return-to-Center steering lets you maneuver orderpicker by rotating handle one-quarter of a circle.  Eliminates need to turn a traditional wheel lock-to-lock and reliance on visual steer indicator.
· Steering System automatically centers drive tire at every power start-up so operator always knows direction of travel.
· Pin-mounted forks are adjustable to fit variety of pallet sizes.
· Self-adjusting pallet clamp automatically releases its jaws to accept pallet stringer.
· Robotically welded, formed steel fork section provides superior rigidity.
· On-board storage compartments keep work tools close-at-hand.  Removable trash bin helps keep workspace clutter-free and efficient. 
· Standard polyurethane drive tire is durable and offers less steering resistance for easier maneuvering.
· Direct drive power steering provides smooth, quiet and precise steering.

Service

· Single piece ABS service compartment hood is easily removed by loosening 4 quarter turn fasteners.
· Two steel hinged doors reveal an uncluttered compartment which makes all components easily visible and within reach for quick servicing.
· CAN communications provide on-board capability for truck set-up, parameter adjustments, and diagnostics using the display gauge and system inputs.  No handset, laptop or password needed.  Over-the-mast cable only has 8 conductors (in lieu of the 27 conductors on previous model) regardless of option mix for increased reliability.  
· Backlit gauge combines hour meter, BDI, and fault code messaging capabilities into one compact display.
· External sight glass permits visual inspection of hydraulic fluid without need to open compartment doors or remove filler cap.
Service cont.
· Battery compartment is accessible from both sides through convenient, easily removed side panels.  Large 2.5-inch diameter rollers allow easy battery access for maintenance checks and removal.  
· Trunnion-mounted mast makes it easier to remove mast for shipping or service work.
· Adjustable side thrust wear plugs help maintain zero clearance between them and the mast channel at the tightest point.  They help keep the channel in the center position.  An adjustment tool is available to make wear plug adjustment easier.
· Drive tire is easily removed by loosening five lug nuts.
· Single bolt load wheel installation simplifies load wheel replacement (one bolt per wheel). 
· Electrical wiring is numbered for quick circuit tracing.
· Six grease fittings on entire truck:  2 on master drive unit bearing and 4 on platform thrust rollers.
· Direct drive power steering eliminates the maintenance and servicing associated with chain type systems.
Ergonomics

· Large-sized platform provides 27.5” deep x 40” wide working space at foot level.  
· One-inch thick floor mat cushions operator’s feet yet provides right amount of firmness for sure footing at high elevations.
· Gas spring-assisted retractable sidegates (optional on R30XMS2) provide side protection for operator.  This promotes a feeling of security and stability when working at higher elevations.
· Wire mesh screen, overhead 2-speed fan and optional full body fan work together to promote a comfortable work environment.
· Flush mounted brake switch eliminates potential trip point. 
· Ergonomically located controls and instrumentation promote easy interactive relationship between operator and orderpicker.
· Return-to-Center steer handle is covered with soft-touch material for a comfortable grip.
· Ergonomically designed accelerator handle is mounted at 45 angle to match operator’s natural forearm posture for a comfortable grip.  
· 3-position detent accelerator handle and optional adjustable console allow operators of varying heights and stature to assume the most comfortable driving position.
· Auto Deceleration System (ADS) slowly brings orderpicker to a smooth stop.
Application Specific Offerings / Optional Equipment


· VISTA 3-stage masts are available with maximum fork heights up to 23-feet (25 feet through SPED). Note: Refer to the SPED price book for masts with free lift and other mast options.
· Orderpicker can be programmed to stop overhead guard height from interfering with lowest obstruction in picking area.  Capability available with mast lift limit option.
· Orderpicker can be programmed to restrict the maximum fork height but allows ability to override governed height with the mast lift limit override option.
· Optional mast lower override allows operator to lower forks beyond pre-set limit.  This option is typically equipped on orderpickers if they are primarily handling picking carts or baskets.
· Optional 3-stage, zero free lift mast with a 300” maximum fork height is available through SPED. Consult SPED Price Book and/or Application Engineering.
· Optional platform widths (48”, 54” or 60”) extend the working room as much as 10–inches on each side. 
· Optional Lexan shield is available as a SPED alternative to the standard wire mesh screen. Consult SPED Price Book and/or Application Engineering.
Application Specific Offerings / Optional Equipment

· Steel or aluminum auxiliary platforms are available in various sizes through SPED. Platforms slide onto forks.  They are used when picking loads longer than a pallet.   Most often, this option is utilized in the furniture industry.  Note:  Platforms reduce lifting capacity.   Consult SPED Price Book and/or Application Engineering.
· Adjustable console option allows console to be height-adjustable up to 6-inches so controls are at a comfortable reach.
· An optional base width (48”) provides a wider truck footprint for improved stability for fork heights above 213”.  
· Two adjustable spotlights can be added to standard light and fan package as an option. These spotlights provide extra illumination of load areas, aisle ways, and bins. 

· Fixed hoop side rails are offered as an option to the standard retractable side gates.  These rails are welded to platform upright, which eliminates the need for traction cutout compared to the standard offering.

· Optional 4-post type overhead guard is available through SPED.  Consult SPED Price Book and/or Application Engineering.
· Safety tethers are available in different styles to suit operator preferences.  Options include:  tether line with medium size belt (waist size 36 to 44); retractable tether with medium size belt; tether with full body harness; or retractable tether with full body harness.
· Additional fork lengths (36”, 42”, 48”, 54” or 78”) are available to accommodate different load lengths.
· Optional Siped polyurethane drive tire is available to match customer floor requirements.
· Freezer option allows truck to work continuously in temperatures to -20º Fahrenheit.  
· Optional multi-turn steering offers an alternative to return-to-center steering.   Audible alarm sounds if truck is over steered.  Advantageous option if customer has a mixed fleet of orderpickers equipped with multi-turn steering.  

· Optional base arm guide rollers are necessary for truck operation in rail-guided aisles.

· Truck can be ordered without pallet clamp.  Most often, this option is ordered when orderpicker is carrying non-palletized loads such as bins.

· 36 volt power option provides needed power boost for high cycle, high productivity picking operations.

· Twelve-volt power supply option is available for accessory equipment such as RF scanners.  Consult SPED Price Book and/or Application Engineering.
· Optional UL Type EE construction is required if orderpicker is working in locations where volatile, flammable liquids or gases and ignitable fibers are present.  Typical EE batteries with lockable covers are not required since the truck equipped with the EE option has lockable battery covers. 

· Optional wire guidance package is available for  6.25 or 5.25 kHz frequencies for compatibility with various manufacturers’ systems.
· High-level traction option permits traction above 212” while in the aisle.
· Optional 16.6” wide battery compartment available through SPED.  Consult SPED Price Book and/or Application Engineering.  Note: Batteries exceeding specified maximum amp hour rating will void UL. 
· Optional 60” pin-type fork length is available through SPED.  Consult SPED Price Book and/or Application Engineering.
· Optional toggle ignition (keyless entry) is available through SPED. Option replaces standard key switch.     Consult SPED Price Book and/or Application Engineering.
· Audible, motion, or backup alarms are available through SPED.  Consult Guide for Users of Industrial Trucks brochure to help determine the appropriateness of these audible and signaling devices.  Also, consult SPED Price Book and/or Application Engineering.
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