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Summary of R30XM2 FAB Statements

 

	PRODUCT REPORT CARD

	 
	Hyster

	INCREASED PRODUCTIVITY
	(

	· State-of-the-art separately excited motor (SEM) technology

· HySenseTM continuous height sensing system optimizes maximum travel speed at various fork heights.

·  Accelerator handle provides simultaneous control of lift/lower, travel direction, speed, and horn functions

·  Variable lift/lower speed control

· Available in standard 24-volt or optional 36-volt electrical system for job matched performance.
	 

	INCREASED OPERATOR COMFORT
	(

	· Spacious operator platform

· Anti-fatigue platform floor mat

· Gas-spring assisted swing-up side rails for side protection

· Ergonomically located controls for operating ease

· Widely-spaced 3 stage mast channels and wire mesh safety screen improve view ahead

· Cushioned platform stops
	 

	REDUCED PRODUCT DAMAGE
	(

	· Variable lift/lowering for stable load handling

· Lock-tight pallet clamp secures load

· Auto Deceleration System (ADS) for smooth controlled stops
	 

	RELIABILITY/DEPENDABILITY 
	(

	· Reliable CANbus: serial communications network link

· Non-contact sensors: hall effect and optical encoders

· Steel nose guard protects load wheels

· Stationary traction motor with direct drive steer system

· UL Type E approval

· Competitive truck warranty: 12 months or 2,000 hours from date of installation
	 

	ENHANCED SERVICEABILITY
	(

	· Clutter-free service compartment layout

· Simplified wiring with sealed in-line connectors

· Single point diagnostic capability – no laptop, handset or password needed

· Minimal service intervention

· Trunnion-mounted 3 stage Vista Mast
	 

	REDUCED MAINTENANCE COSTS
	(

	· Single eight conductor over-the mast cabling

· Easy access to motor brushes

· On-board diagnostics
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