
Hyster Gas Cushion

S40XM, S50XM, S60/65XM

Performance

· S40-65XM has a Mazda 2.0L engine standard with the Mazda 2.2L and GM 3.0L optional. All are 4 cylinder, overhead cam design for high performance, durability, low noise and emissions. 
· Hyster VISTA Mast features full-face, canted load rollers allowing full-face roller contact with mast channels, cushioning between stages

· Six load roller carriage with tapered bars for greater visibility at second rack level in a warehouse. 
· Forks are upset forged from single piece of high strength steel – extra metal is provided at bend for wear resistance
· Powershift transmission is controlled by electric solenoid, has built-in accumulator for reduced component stress – Transmission cooler located in the radiator
· Self-energizing, Duo-servo brake system which requires less pedal effort to stop the forklift
· Full-floating drive axle supports mast trunnion mountings and service brake assemblies
· Hydraulic pump is driven by direct connection to the engine crankshaft, which provides for less parts to maintain
· Lift and tilt cylinders are chrome plated and are equipped with wiper rings to help prevent damage
Service

· Engine compartment hood and side open to allow excellent access to engine and operator check points
· Floorplate lifts off without tools to provide easy access to pedal linkages and transmission dipstick
· Steer axle is provided with grease fittings at key points to increase life
· Hyster VISTA Mast is designed to be wear resistance, through canted roller bearing, increasing service life
Ergonomics

· Mounted step is a low 17” from the ground and is integral to the truck’s frame
· Molded Handgrip is mounted on the left front overhead guard leg (Optional right side handgrip)
· Standard Seat is covered in soft vinyl; Premium full-suspension seat is optional – both adjust between 2.3 and 4.8 inches fore and aft
· Steering column tilts to five positions
· Hydraulic control levers are located to the right of the operator and have molded grips
· Adjustable parking brake handle requires low force to engage/release. Grip is contoured to operator’s hand
· Instrument panel includes hour meter, engine coolant temperature and fuel level gauges (gas trucks only) and engine oil pressure, battery charging indicator, transmission temperature and seat belt reminder warning lamps. Brake fluid level and low coolant level warning lamps are optional 
· Convenience Box is included to hold clip boards, pens and pencils
· Two pedal design includes accelerator pedal and combination brake/inching pedal
· Low noise and vibration due to suspended operator compartment and sound deading material in the engine compartment

Application 

· Three spool valve is standard, Fourth spool is available as an option
· Sideshifter is available as an option
· Many optional light packages are available such as headlights, turn signals, adjustable work lights and flashing lights
· Dust protection, foundry protection and an anti-clog radiator are available as options
· GS and LPS ratings are available for necessary applications
· Tire options include non-marking, poly and a wide drive tire option
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